## State Documentation Index

# Hadron state description sheet

## State title

fxStoptime

## Type of sound

Midi triggered “stop time” or “hold” effect. Audio will pass thru Hadron even when no midi notes are sent to it. When Hadron receives a midi note, it will hold the current audio signal until the midi note is released. Maximum hold time is approximately 12 seconds.

## Controllers

Expression1: Time Stop Amount. Full stop when control is at zero, slow down time when the control is increased
Expression2: Time LFO Amount, a slowly modulating time pointer activated during time stops
Expression3: Time jitter, a random modulation of the time pointer during time stops
Expression4: Grain Duration, adjust to fit the type of audio input material. Longer durations will generally give a smoother time stop

## Midi keyboard control

Any midi note input triggers the “stop time” processing.

## Suggested source waveform

Slot1: audioInput
Slot2: Not used
Slot3: Not used
Slot4: Not used

Waveform sources/slots used: 1

## Pitch definition mode

Not applicable