## State Documentation Index

# Hadron state description sheet

## State title

grDualFmThin

## Type of sound

Combined grain rate FM and grain pitch FM. Continuous (unstepped) function for modulation frequency, so the frequency deviations will create vibratos and inharmonicities. Grain rate mod index is kept withing range where pitch is stable.

## Controllers

Expression1: Grain Pitch FM Frequency, unstepped, octave range.
Expression2: Grain Pitch FM Index
Expression2: Grain Rate FM Frequency, unstepped, octave range.
Expression4: Grain Rate FM Index

## Midi keyboard control

Note Number: Pitch
Velocity: Amp

## Suggested source waveform

Slot1: Sine, other waveforms may be used for a more aggressive timbre
Slot2: Not used
Slot3: Not used
Slot4: Not used

Waveform sources/slots used: 1

## Pitch definition mode

Grain Rate
Octave: +2
e.g.
440Hz at note num 69 = octave 0
220Hz at note num 69 = octave -1