## State Documentation Index

# Hadron state description sheet

## State title

fxSyncDelayPitch

## Type of sound

Tempo synced Grain Delay pattern with separate pitching of each delay tap (voice).

## Controllers

Expression1:
Pitch scaling, continuous from zero to:
Voice1: no transposition
Voice2: up 3 semitones
Voice3: up one octave
Voice4: down 7 semitones
Expression2:
Time scaling (delay time):
Voice1: half note
Voice2: dotted quarter
Voice3: quarter note
Voice4: dotted 8th
Note: the delay time is modified using a transfer function.
The first 50% of the slider affects the delay time in continuous manner from 0 to 50% of the above.
After this, it will proceed in steps (half note, triplet and whole note).
Expression3:
Grain Delay Feedback
Delay effect feedback (be careful when Expression 1 is at zero at it will overdrive feedback)
Expression4:
Wave(Voice) Mix
at 0%: Voice1 only
at 25%: Voice1&2
at 50%: Voice2&3
at 75%: Voice3&4
at 100%: All

## Midi keyboard control

Midi input not used for parameter control.

## Suggested source waveform

Slot1: audioInput
Slot2: audioInput
Slot3: audioInput
Slot4: audioInput

Waveform sources/slots used: 1,2,3,4

## Pitch definition mode

Not applicable