## State Documentation Index

# Hadron state description sheet

## State title

fxSnapper

## Type of sound

Rhythmic “snapping” texture. Each sound particle is routed separately to stereo left/right and to internal bandpassfilters. Timbral animation (wavemix) by LFO and by note number modulo.

## Controllers

Expression1: Grain rate mod (tempo)
Expression2: Transposition, original pitch at 0%, down 2 octaves at 50%, then up one octave at 100%
Expression3: Modification of output routing (channel masks). Bandpass frequency (increase) and bandwidth (decrease)
Expression4: Grain delay time, also splitting into three separate echoes (delay times)

## Midi keyboard control

Midi input not used for parameter control

## Suggested source waveform

Slot1: audioInput
Slot2: audioInput
Slot3: audioInput
Slot4: audioInput

Waveform sources/slots used: 1,2,3,4

## Mask tables

Channelmask:
A: Left, Right, Bandpass1, Bandpass2 (loop length=4 particles)
B: Left, Right, BP1, BP2 BP1, Right, BP22 (loop length=7 particles)

## Pitch definition mode

Not applicable.