## State Documentation Index

# Hadron state description sheet

## State title

fxSprayDelayPitch

## Type of sound

Tempo synced Grain Delay with 4-voice pitching and grain spray.
Voice pitching is set to:
Voice1: no transposition
Voice2: up 3 semitones
Voice3: up one octave
Voice4: down 7 semitones

## Controllers

Expression1:
Grain Spray: delay time deviation, grain rate and channelmasking
Channelmask morphing starts at 75%
Expression2:
Time scaling 0 to 100% of:
Voice1: half note
Voice2: dotted quarter
Voice3: quarter note
Voice4: dotted 8th
Expression3:
Grain Delay Feedback
Delay effect feedback (active when Expression1 is at max)
Expression4:
Wave(Voice) Mix
at 0%: Voice1 only
at 25%: Voice1&2
at 50%: Voice2&3
at 75%: Voice3&4
at 100%: All

## Midi keyboard control

Midi input not used for parameter control.

## Suggested source waveform

Slot1: audioInput
Slot2: audioInput
Slot3: audioInput
Slot4: audioInput

Waveform sources/slots used: 1,2,3,4

## Mask tables

Channelmask:
A: Left, Right, (loop length=8 particles)
B: Left, Right, BP1, BP2, LP, BP3, Delay L, Delay R (loop length=8 particles)

## Pitch definition mode

Not applicable